{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"flags":["formulas_cached_only"]}
["Aseptic tank volume & utility consumption"]
["Aseptic Tank L",{"v":7000,"d":"7,000"},{"v":12000,"d":"12,000"},{"v":20000,"d":"20,000"},{"v":30000,"d":"30,000"},{"v":40000,"d":"40,000"},{"v":50000,"d":"50,000"}]
["Working volume",{"v":5500,"d":"5,500"},{"v":10800,"d":"10,800"},{"v":18700,"d":"18,700"},{"v":26500,"d":"26,500"},{"v":36000,"d":"36,000"},{"v":45700,"d":"45,700"}]
["Steam Supply (kg/h)",620,770,{"v":1100,"d":"1,100"},{"v":1600,"d":"1,600"},{"v":2100,"d":"2,100"},{"v":2600,"d":"2,600"}]
["Steam Consumption (kg)"]
["Pre-sterilization (2.7 bar)",130,160,220,310,460,620]
["Steam barrier (1.0 bar)",30,30,30,30,30,30]
["Cooling Water Supply (L/h)",{"v":9500,"d":"9,500"},{"v":10000,"d":"10,000"},{"v":11000,"d":"11,000"},{"v":15000,"d":"15,000"},{"v":17500,"d":"17,500"},{"v":20000,"d":"20,000"}]
["Cooling Water (20°C) Consumption"]
["Post-sterilization (L)",{"v":1400,"d":"1,400"},{"v":1800,"d":"1,800"},{"v":2000,"d":"2,000"},{"v":3000,"d":"3,000"},{"v":4000,"d":"4,000"},{"v":5000,"d":"5,000"}]
["Compressed Air, 6 bar (L/min)",55,55,55,55,55,55]
["Clean Air Consumption (Nm3/h)",40,65,120,160,210,250]
["Compressed Air Receiver, 6 bar (m3)",1.5,2.5,2.5,3.5,4.5,5.5]
["CIP Flow (L/h)",{"v":15000,"d":"15,000"},{"v":15000,"d":"15,000"},{"v":15000,"d":"15,000"},{"v":22000,"d":"22,000"},{"v":25000,"d":"25,000"},{"v":25000,"d":"25,000"}]
[]
["Aseptic Tank Dimensions"]
["Aseptic tank","Vessel diameter","Width","Overall height","Outlet height","Weight"]
["7,000L","2,100mm","3,100mm","4,300mm","600mm","2,000kg"]
["12,000L","2,500mm","3,500mm","5,000mm","600mm","3,000kg"]
["20,000L","3,100mm","4,200mm","5,300mm","700mm","4,500kg"]
["30,000L","3,600mm","4,700mm","5,500mm","700mm","6,000kg"]
["40,000L","3,600mm","4,700mm","6,300mm","700mm","8,800kg"]
[]
["产品属性参数"]
["After-sales Service:","Video Technical Support, Online Support"]
["Warranty:","1year"]
["Process:","Sterile processing"]
["Power source:","Electric"]
["certification","CE, ISO9001"]
["Automation level:","Automatic"]
["Application:","Dairy/Beverage/Brewery/Food/Juice"]
["Whether to customize:","Customized"]
["Transport packaging:","Export Wooden box"]
["Specifications:","Can be customized"]
["Trademark:","RENOX "]
["country of origin:","WUXI,CHINA"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}